ctd_con_report.txt :

Configuration and calibration information (from *.con file) for various sensors on 
the profiling CTD [SBE 25] on the R/V SAVANNAH

** Configuration and setup were the SAME for ALL Long Bay Cruises [ Sep 2011 - Apr 2012 ]

---------------------------------------------

EXAMPLE :
Instrument configuration file: C:\SAV-12-03\SAV1203_STA01.CON

Configuration report for SBE 25 Sealogger CTD
---------------------------------------------

External voltage channels  : 5
Firmware version           : Version >= 2.0
Real time data output rate : 1 scan/sec
NMEA position data added   : Yes
NMEA depth data added      : No
NMEA time added            : No
NMEA device connected to   : deck unit
Surface PAR voltage added  : No
Scan time added            : No

1) Frequency 0, Temperature

   Serial number : 2336
   Calibrated on : 24 Sep 2009
   G             : 4.34734821e-003
   H             : 6.43102186e-004
   I             : 2.33928800e-005
   J             : 2.23819928e-006
   F0            : 1000.000
   Slope         : 1.00000000
   Offset        : 0.0000

2) Frequency 1, Conductivity

   Serial number : 1909
   Calibrated on : 25 Sept 2009
   G             : -4.05908821e+000
   H             : 5.10130528e-001
   I             : -1.06351858e-003
   J             : 8.05364735e-005
   CTcor         : 3.2500e-006
   CPcor         : -9.57000000e-008
   Slope         : 1.00000000
   Offset        : 0.00000

3) Pressure voltage, Pressure, Strain Gauge

   Serial number : 0715
   Calibrated on : 13Apr11
   A0            : 5.433286e+002
   A1            : -1.516003e-001
   A2            : 6.575976e-008
   Offset        : 0.00000

4) A/D voltage 0, Fluorometer, WET Labs WETstar

   Serial number : WS3S 1021P
   Calibrated on : 23 Dec 2010
   Vblank        : 0.067
   Scale factor  : 15.000

5) A/D voltage 1, Fluorometer, WET Labs CDOM

   Serial number : WSCD 962P
   Calibrated on : 15 August 2011
   Vblank        : 0.082
   Scale factor  : 21.500

6) A/D voltage 2, User Polynomial

   Serial number : BBRT-305
   Calibrated on : 3 Nov 08
   Sensor name   : WETLabs Backscatter Meter
   A0            : -0.06252100
   A1            : 1.03000000
   A2            : 0.00000000
   A3            : 0.00000000

7) A/D voltage 3, Oxygen, SBE 43

   Serial number : 0639
   Calibrated on : 22 Sept 09
   Equation      : Sea-Bird
   Soc           : 3.61900e-001
   Offset        : -4.86300e-001
   A             : -9.80530e-004
   B             : 1.72270e-004
   C             : -3.12670e-006
   E             : 3.60000e-002
   Tau20         : 1.42000e+000
   D1            : 1.92630e-004
   D2            : -4.64800e-002
   H1            : -3.30000e-002
   H2            : 5.00000e+003
   H3            : 1.45000e+003

8) A/D voltage 4, PAR/Irradiance, Biospherical/Licor

   Serial number        : SPQA 4175
   Calibrated on        : 13 July 2011
   M                    : -0.77180265
   B                    : -3.53714840
   Calibration constant : 4.50000000
   Multiplier           : 1.00000000
   Offset               : 0.00000000

Scan length                : 46
